OPERATING INSTRUCTIONS FOR **DCU**

* RIGHT CLICK THE DCU MONITORING CLIENT ICON IN THE DESKTOP, CHOOSE RUN AS ADMINISTRATOR PRESS ENTER CHOOSE YES
* IT WILL ASK THE USER AND PASSWORD

(USER: AMR PASS: 123) CLICK **LOGIN.**

* THEN SELECT **METER RESDING PANELS** TO ACCESS REVENUE METER READINGS.
* THEN SELECT **METER ID** AND CHOOSE **THE METER NAME** TO GET THE SPECIFIC READING OF THE CHOOSEN METER (INSTANTANEOUS READING, COMSUMPTION READING, MAXIMUM DEMAND READINGS, METER SCEURITY READINGS.)
* SELECT THE **PQ READING PANELS** TO ACCESS PQ READINGS (INSTANTANEOUS READINGS, CONSUMPTION READINGS, PRESENT & PEAK INTERVAL DEMAND, MAXIMUM/MINIMUM READINGS, HARMONICS READINGS, SER) CHOOSE 3PH, 1PH AT THE BOTTOM OF EACH PARAMETER)
* SELECT **NW HEALTH/EVENTS** TO ACCESS THE EVENTS OCCURRED.
* DOUBLE CLICK **(LAUNCH DCU DATA VIEWER)** TO VIEW CONSUMPTION & LOAD PROFILE REPORTS.
* CHOOSE (THE SUBSTATION NAME, METER NAME AND REPORT) TO VIEW THE SPECIFIC METER’S REPORTS.
* OPERATING INSTRUCTION FOR **REVENUE METER**
* USE LEFT LAST ARROW TO SCROLL 10 SCREENS BACKWARD.
* USE SECOND ARROW TO SCROLL ONE SCREEN FORWARD.
* USE THIRD ARROW TO SCROLL ONE SCREEN BACKWARD.
* USE RIGHT LAST ARROW TO SCROLL 10 SCREENS FORWARD.
* SCREEN NO. 1 – 90 REPRESENTS 0 – 8 TARIFF’S
* SCREEN NO. 91 – 146 REPRESENTS OTHER PARAMETERS ( VOLTAGE, CURRENT, POWER FACTOR, REACTIVE POWER, APPARENT POWER, MAXIMUM DEMAND,…. ETC)