**CT SECONDARY INJECTION TEST:**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PHASES** | **INJECTED**  **CURRENT**  **(A)** | **LCC PANEL – D08** | | **PROTECTION PANEL - D08+RP** | | | | | |
| **CT TERMINAL BLOCK** | | **TEST SWITCH** | | **MAIN RELAY** | |
| **R** | **0.250** | **X26A : 42** |  | **1X1 : 1** |  | **TS1 : 13A** |  | **X401 : 1** |  |
| **Y** | **0.500** | **X26A : 47** |  | **1X1 : 3** |  | **TS1 : 14A** |  | **X401 : 3** |  |
| **B** | **0.750** | **X26A : 52** |  | **1X1 : 5** |  | **TS1 : 15A** |  | **X401 : 5** |  |
| **N** | **--** | **X26A : 56** |  | **1X1 : 7** |  | **TS1 : 16A** |  | **X401 : 6** |  |

**MAIN RELAY MEASUREMENT:**

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PHASES** | **INJECTED**  **CURRENT**  **(A)** | **MAIN RELAY**  **MEASUREMENTS** | |  | | | | | |
| **PRIMARY** | **SECONDARY** |  | |  | |  | |
| **R** | **0.250** |  |  |  |  |  |  |  |  |
| **Y** | **0.500** |  |  |  |  |  |  |  |  |
| **B** | **0.750** |  |  |  |  |  |  |  |  |
| **N** | **--** |  |  |  |  |  |  |  |  |