|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GENERAL DATA AND INFORMATION:  |  |  | | --- | --- | | Bay No. | **DCDB#** | | Designation |  |  MECHANICAL CHECKS AND VISUAL INSPECTION:  |  |  |  | | --- | --- | --- | | ITEM | DESCRIPTION | CHECKED | | 1 | Inspect for any physical damage or defects. |  | | 2 | Verify connections as per approved drawing |  |   **Secondary Injection Test :** Ammeter Scale [ 0 – 180 A ]   |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Current %** | **Injected Current (A)** | **Observed meter**  **reading (A)** | **% Error** | **Remarks** | | 25 |  |  |  |  | | 50 |  |  |  |  | | 75 |  |  |  |  | | 100 |  |  |  |  |   % Error = (Observed meter reading-Applied meter reading) / Full scale reading x 100.   * Test Equipment's : FREJA 300 |