|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| GENERAL DATA AND INFORMATION:  |  |  |  |  |  | | --- | --- | --- | --- | --- | | LOCATION |  |  | MANUFACTURER | ***Bowthorpe EMP*** | | PHASE | B – Phase |  | MODEL no. | SC13 | | COUNTER SCALE | 0 - 50 mA |  |  |  |  2. MECHANICAL CHECKS AND VISUAL INSPECTION:  |  |  |  | | --- | --- | --- | | ITEM | DESCRIPTION | CHECKED | | 1 | Inspect for any physical damage or defects. |  | | 2 | Verify nameplate information for correctness |  | | 3 | Check tightness of all bolted connections. |  |  3. ELECTRICAL TESTS:  |  |  |  |  | | --- | --- | --- | --- | | COUNTER SCALE | MEASURED VALUES | ERROR % | REMARKS | | 1 |  |  |  | | 2 |  |  |  | | 3 |  |  |  | | 10 |  |  |  | | 30 |  |  |  | | 50 |  |  |  | |